**Frostoberfest 2022**

Pure Stocks:

We will allow cars to run from other tracks with their rules but must conform to following rules for an equal and fair playing field.

All cars including Flamboro cars.

Cars originally equipped with diagnostic port must have working diagnostic port.

ECM must be stock with stock settings.

\*\*\*No ECM reprogramming.

Engine and transmission must be stock for year, make and model.

Camber maximum 2" on right and left front.

Camber maximum 1/2 on right and left rear to allow for bent parts.

Measured at top and bottom of rim.

Springs must be equal side to side.

No progressive rate front springs.

No lowering or cut springs

\*\*\*No excessively worn springs that lower ride height.

No cars over 180hp factory specs allowed

Only right front racing rim allowed all other rims must be stock or stock backspace.

One way radio mandatory 454 frequency

Tires must be 400 treadwear or higher. Right after race rim on right side.